Reading Random Coil Shifts from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/randcoil.tab
Reading RC Adjustments from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/rcadj.tab
Reading Previous Residue RC Adjustments from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/rcprev.tab
Reading Next Residue RC Adjustments from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/rcnext.tab
Reading Secondary Shift Limits from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/sslimit.tab
Reading Homology Values from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/homology.tab
TALOS Weight Factors from /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/weight.tab
Reading /minnow/bbee/Rosetta_Server_V3/apps/nmrpipe/install/talos/tab/talos.tab, 22839 Triplets
 Clipped  21 E  CA Secondary Shift:    4.790 Limit:    4.660
 Clipped  23 T  CA Secondary Shift:    6.760 Limit:    4.660
 Clipped  26 L   C Secondary Shift:    4.810 Limit:    3.727
 Clipped  33 V  HA Secondary Shift:    1.330 Limit:    1.047
 Clipped  36 T  HA Secondary Shift:    1.160 Limit:    1.047
 Clipped  36 T  CA Secondary Shift:   -7.980 Limit:   -3.445
 Clipped  37 P   C Secondary Shift:   -3.571 Limit:   -3.070
 Clipped  37 P  CA Secondary Shift:   -2.270 Limit:   -2.220
 Clipped  40 G  HA Secondary Shift:   -1.785 Limit:   -0.999
 Clipped  41 M  HA Secondary Shift:   -1.240 Limit:   -1.080
 Clipped  48 Y  CA Secondary Shift:    5.190 Limit:    4.660
 Clipped  54 T  CA Secondary Shift:    5.720 Limit:    4.660
 Clipped  58 R   C Secondary Shift:    4.820 Limit:    3.727
 Clipped  68 I  CA Secondary Shift:   -3.930 Limit:   -3.445
 Clipped  84 A   C Secondary Shift:    5.126 Limit:    3.727
 Clipped  92 I   N Secondary Shift:  -12.615 Limit:  -11.301
 Clipped 103 F  CA Secondary Shift:    6.620 Limit:    4.660
 Clipped 108 T  HA Secondary Shift:    1.050 Limit:    1.047
 Clipped 109 V  HA Secondary Shift:    1.360 Limit:    1.047
 Clipped 113 G   C Secondary Shift:   -3.950 Limit:   -3.725
 Clipped 117 T   N Secondary Shift:  -16.079 Limit:  -11.301
 Clipped 118 V   N Secondary Shift:  -11.704 Limit:  -11.301
 Clipped 125 D  CA Secondary Shift:   -3.670 Limit:   -3.445
 Clipped 130 I   N Secondary Shift:  -12.790 Limit:  -11.301
 Clipped 137 E  HA Secondary Shift:   -2.050 Limit:   -1.080
 Clipped 138 V  HA Secondary Shift:   -1.930 Limit:   -1.080
 Clipped 139 W   N Secondary Shift:  -14.215 Limit:  -11.301
 Clipped 148 K  HA Secondary Shift:    1.500 Limit:    1.047
 Clipped 158 V  CA Secondary Shift:   -3.450 Limit:   -3.445
 Clipped 160 N  CA Secondary Shift:   -3.760 Limit:   -3.445
 Clipped 172 F  HA Secondary Shift:    1.063 Limit:    1.047
 Clipped 177 A   C Secondary Shift:    4.246 Limit:    3.727
 Clipped 179 V  CA Secondary Shift:    5.050 Limit:    4.660
 Clipped 186 L   C Secondary Shift:    4.200 Limit:    3.727
CA vs CA-CB (negative, 0), offset:      nan   fitting error:      nan
CB vs CA-CB (negative, 0), offset:      nan   fitting error:      nan
HA vs CA-CB (negative, 0), offset:      nan   fitting error:      nan
 C vs CA-CB (negative, 0), offset:      nan   fitting error:      nan
